**B’s FAB Polaris Xpedition Driving Light Kit Instructions**

**KIT INCLUDES**

* 2 - LED lights
* 1 - Mounting bracket
* 2 - Speed nuts
* 2 -Bolts
* 1 - Y-harness
* 1 – (Optional) OEM switch

1. Remove grill and hood
2. Remove bumper, there are 2 lower bolts and 4 upper bolts
3. Remove the front fascia, 4 push pins and 2 bolts
4. Remove both light hole covers from backside of front fascia
5. Install speed nuts onto the lower front fascia as shown below

A close up of a keyboard

AI-generated content may be incorrect.

1. Install driving lights onto bracket and bolt bracket into fascia as shown below

A close-up of a black car bumper

AI-generated content may be incorrect.

1. Install & route wiring into backside of fascia as shown below and zip tie into place, leave the end of the Y harness loose on drivers’ side

A close-up of a keyboard

AI-generated content may be incorrect.

1. Locate existing plug near bottom of radiator as shown in pic below, remove dust cap from existing plug and plug into Y connector and reinstall fascia back onto machine

A close up of a radiator

AI-generated content may be incorrect.

1. Switch installation - if optional switch was purchased. Remove switch cover plate next to factory headlight switch. Locate red switch plug by looking through switch hole and plug switch into the plug. Push switch into opening, you will hear it click into place
2. Aim lights as desired.

Thank You!

We really appreciate your business, and your satisfaction is very important to us. If you are not satisfied, we ask you please contact us so can resolve any issues or concerns you may have.

Web – www.bsfabutv.com

Email – info@bsfabutv.com

Phone – 1-888-779-1497